Go to the tablet to manage fuel and loading

1- **Bat 1** and **Bat 2** ON

2- Exit power

3- Align the addirs (**ADR1, ADR2, ADR3**) to NAV

4- Put the **DUME** in the middle

5- **AWLT** right next to the **DUME** to test all the cookpit lights

6- the **EMER EXIT LT** to ON

7- Put the **NO SMOKING** next to **EMER EXIT LT** on ON

8- The **SEATBELTS** (close to **NO SMOKING**) we put them on AUTO

9- We can test the APU fire protection system (click on test in the center)

10- Turn on the pumps: **L TK PUMPS 1** and **2, PUMP 1, PUMP2, R TK PUMPS 1** and **2**

11- We set the **NAV &LOGO** to 1

12- We put the **MASTER SW** to ON

13- After some time click on **START** just below

14- We put the **PROBE / WINDOW HEAT** to ON

15- **API BLEED** is set to ON: **PACK 1** and **PACK 2** will be activated

16- Configuration of the FMS and we will finish the loading

17- Finally **EXIT PWR**

18- We will put the **SEATBELTS** on ON